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This document describes the cross sectional diagrams and some further information that may be useful. 
The enclosed section drawings show the size, position and opening mechanisms of the windows that are to be installed.  There are three types of windows to be installed as part of this project
A. Sliding sash windows
B. Fixed mullion windows
C. Mullion windows with an opening mechanism
As advised by the local authority we are providing an example for each type of window that as well as the technical details of the unit, shows the position that the unit will be installed compared to the existing ones.
Drawings 1 and 2 show the existing and proposed windows for the first floor window at the front elevation. This design and positioning will be replicated for the other sliding sash windows on the ground floor and 2nd floor of the front elevation – as described in our initial application and shown in the plans. 
Drawings 3 is the existing fixed mullion window in the centre of the set of 3 mullion windows, on the 1st floor of the rear elevation.  
Drawing 4 is the proposed fixed mullion window on the right hand side of the 3 mullion windows, on the 1st floor of the rear elevation.  
Drawing 5 is the existing opening mullion window on the right hand side of the 3 mullion windows, on the 1st floor of the rear elevation.  
Drawing 6 is the proposed opening mullion window in the centre of the set of 3 mullion windows, on the 1st floor of the rear elevation.  
Please note that because the ground floor at the rear is described as the basement in this application (the house is on a slope), the first floor is the top floor of the rear section of the house.  
The design, size and positioning of the existing and proposed mullion windows (all windows on the rear and right elevations) will be the same as those shown in the cross sectional diagrams (drawings 1-6).  The styles of the existing and proposed for each mullion window is shown in our main application, but in all cases is either a fixed mullion window or an opening mullion window as shown in the drawings provided.
We are working with a supplier to only install glazing units that have a U-value of between 1.2 and 1.5 and use the latest insulating technology. This will make the new installation as insulating as possible while retaining the style and character of the original building - supporting Historic England’s climate change strategy. 
